**WEYERHAEUSER FIRE PREVENTION AND RESPONSE PLAN**

**CRITICAL PROTOCOL FOR ALL FIELD OPERATIONS**

Fire Danger Rating System:

LOW: Normal operations permitted

MODERATE: No operations between 1:00 PM and 8:00 PM

HIGH: Operations restricted to before 11:00 AM, fire watch required for 3 hours after shutdown

EXTREME: All operations suspended except by special permit

Prevention Requirements:

- Maintain 5 gallon backpack pumps (1 per employee) at all active operations

- Maintain fire extinguishers on all equipment and vehicles

- Conduct daily fire tool inspections before operations begin

- Clear landing areas of flammable debris within 50ft radius

- Maintain water truck (minimum 500 gallons) at all cable yarding operations

- No smoking except in designated areas

Equipment Specifications:

- All power saws must have approved spark arresters

- Heavy equipment must have fire suppression systems

- No metal-tracked equipment operation on rock surfaces during HIGH or EXTREME conditions

- Radio communications required for all field crews

Response Protocol:

1. Safety of personnel is highest priority

2. Report all fires immediately to:

a. Local fire emergency (911)

b. Company dispatch (ext. 5911)

c. Regional manager

3. Attempt initial attack if safe to do so

4. Document point of origin and preserve evidence

5. All personnel must know location of fire tool cache and evacuation routes

Contact: Fire Prevention Officer (ext. 5134) for questions regarding this protocol